**Enigma functionality test data**

NonRotReflector

1. Set circuitry to [25, 24, 23, 22, 21, 20, 19, 18, 17, 16, 15, 14, 13, 12, 11, 10, 9, 8, 7, 6, 5, 4, 3, 2, 1, 0]

Encrypt the argument when it is run, it should be 25-arg

1. Check that encrypt takes position into account

Set circuitry to [